****

**European Union Rule of Law Mission in Kosovo**

**EULEX Kosovo**

Ndertesa Farmed

“Muharrem Fejza” p.n.

Lagja e Spitalit

10000 Pristina, Kosovo

[www.eulex-kosovo.eu](http://www.eulex-kosovo.eu)

**CLARIFICATIONS No. 1**

1. **PUBLICATION REFERENCE: PROC/848/18/Supply of Construction Materials No. 6- - Questions regarding the Tender Dossier, Technical Specifications-** **Lot 6 Electrical Material**

|  |  |  |
| --- | --- | --- |
| Question  No | Question | Answer |
| 1 | Is it okay for you as a Contracting Authority to convert the cable signatures an specifications into the equivalent Italian Standard? | Kindly be informed that the EU norms/standards should be respected. As stipulated under Article 11 of the Instruction to Tenderers: *For LOT 6: Electrical material must be CE marked*.  Please refer to Corrigendum no.1. |
| 2 | In some cable types, you ask for the wires to be unique. Will be taken into account flexible multi-thread norms? | Please note that all cables specified in the technical specifications have to be in accordance with EU norms/standards. As stipulated under Article 11 of the Instruction to Tenderers: *For LOT 6: Electrical material must be CE marked*.  Please refer to Corrigendum no.1. |
| 3 | In the switch-plug series do you have modular series applied or not? | There is no modular specified. |
| 4 | The variant of circular or square boxes will be used in the switch-plug series ? | Circular boxes will be used in the switch-plug series. |
| 5 | Regarding to the specified projectors (floodlights), one of the technical specifications is: -20°C +50°C in relation to the specified projectors, is it a problem that the maximum temperature is +40°C, because the normal European products that we have dont reach  +50°C, otherwise we have to go to a special product. | Kindly note that the ambient temperature range should be as stipulated in the technical specifications:-20…50 °C. Only products specified within the minimum and maximum temperature range, according to the specifications will be consider compliant. |
| 6 | The Led light Surface you ask has the motion sensor inside, the specifications comes out that is a Chinese product. Can we quote a with a non-embedded sensor inside and out of European production. | Please be informed that none of the products have been specified with internal sensors. Please note that the items specified in the technical specifications have to be in accordance with EU norms/standards. As stipulated under Article 11 of the Instruction to Tenderers: *For LOT 6: Electrical material must be CE marked*.  Please refer to Corrigendum no.1. |
| 7 | Given the technical specifications of the switches in general and given our European manufacturers, it seems that some of the technical specifications are in Chinese products. Can we hope for a change in the technical specifications that lead to branded, European Standards? | All technical specifications are according to EU standards and all products should be CE marked and the manufacturer should have an ISO 9001 certificate.  Please refer to the Matrix and to Corrigendum no.1. |